{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["HMI画面变量地址","PLC寄存器地址","PLC物理地址"],"not_rendered":{"charts":0,"images":6,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"HMI画面变量地址","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[[31,0,32,0],[35,0,38,0],[63,0,64,0],[181,0,188,0],[189,0,190,0]]}

{"sheet":"PLC寄存器地址","index":1,"n_rows":548,"n_cols":11,"rows_kept":548,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,5,0,6],[0,9,0,10],[181,4,188,4],[189,4,190,4],[45,9,45,10],[53,9,53,10],[62,9,62,10],[2,9,2,10],[35,4,38,4],[63,4,64,4]]}
[null,null,"D200之后的可读可写，D200之前的只读。标黄表示建议在工控机显示",null,null,"报警",null,null,null,"文本列表"]
["M0000","HMI联机自动命令","D0000",null,null,"S100","液位过低"]
["M0001","调整模式","D0001","操作提示",null,"S101","油温过高",null,null,"操作提示：D1"]
["M0002","手动模式","D0002","动作次数提示",null,"S102","型号非法",null,null,"[1]","调整，请给出命令"]
["M0003","本地自动","D0003","当前模式提示",null,"S103","自动步骤非法",null,null,"[2]","调整，油缸已经上升到位"]
["M0004","联机自动","D0004",null,null,"S104",null,null,null,"[3]","调整，油缸已经下降到位"]
["M0005","手动Mode","D0005",null,null,"S105",null,null,null,"[4]","手动，请给出命令"]
["M0006","自动Mode","D0006",null,null,"S106",null,null,null,"[5]","手动，油缸已经上升到位"]
["M0007","下压次数清零","D0007",null,null,"S107",null,null,null,"[6]","手动，油缸已经下降到位"]
["M0008","Holding","D0008",null,null,"S108",null,null,null,"[7]","本地自动，步骤0，请把油缸退到下极限"]
["M0009","Running","D0009",null,null,"S109",null,null,null,"[8]","本地自动，步骤0，请按下双手启动按钮。"]
["M0010","压力平均值采样计数>","D0010","油缸压力反馈AD-RD3A","RD3A","S110",null,null,null,"[9]","本地自动，步骤1，等待到达慢顶位置。"]
["M0011","压力平均值采样计数=","D0011",null,"RD3A","S111",null,null,null,"[10]","本地自动，步骤2，等待到达压力/位置上限"]
["M0012","压力平均值采样计数<","D0012","油缸压力反馈Float","RD3A","S112",null,null,null,"[11]","本地自动，步骤3，等待保压计时完成"]
["M0013","初始化数据","D0013","油缸压力反馈Float","RD3A","S113",null,null,null,"[12]","本地自动，步骤4，等待泄压计时完成"]
["M0014","故障复位","D0014","油缸压力反馈Mpa","RD3A","S114",null,null,null,"[13]","本地自动，步骤5，等待油缸到达下极限位置。"]
["M0015","存在故障","D0015","油缸压力反馈Mpa","RD3A","S115",null,null,null,"[14]","本地自动，已暂停。"]
["M0016",null,"D0016","油缸压力反馈Bar","RD3A","S116",null,null,null,"[15]"]
["M0017",null,"D0017","油缸压力反馈Bar","RD3A","S117",null,null,null,"[16]"]
["M0018",null,"D0018",null,null,"S118",null,null,null,"[17]"]
["M0019",null,"D0019",null,null,"S119",null,null,null,"[18]"]
["M0020",null,"D0020","油缸压力反馈AD-FromTo","FromTo","S120",null,null,null,"[19]"]
["M0021",null,"D0021",null,"FromTo","S121",null,null,null,"[20]","联机自动，步骤0，请手动把油缸退到下极限"]
["M0022",null,"D0022","油缸压力反馈采样计数","FromTo","S122",null,null,null,"[21]","联机自动，步骤0，等待PLC给出第1次顶出命令。"]
["M0023",null,"D0023","油缸压力反馈采样计数","FromTo","S123",null,null,null,"[22]","联机自动，步骤0，型号2，等待PLC给出第2次顶出命令。"]
["M0024",null,"D0024","油缸压力反馈AD-SUM","FromTo","S124",null,null,null,"[23]","联机自动，步骤0，等待PLC给出第2次顶出命令。"]
["M0025",null,"D0025","油缸压力反馈AD-SUM","FromTo","S125",null,null,null,"[24]","联机自动，步骤0，型号2，等待PLC给出第3次顶出命令。"]
["M0026",null,"D0026","油缸压力反馈AD-Avg","FromTo","S126",null,null,null,"[25]","联机自动，步骤1，等待到达慢顶位置。"]
["M0027",null,"D0027","油缸压力反馈AD-Avg","FromTo","S127",null,null,null,"[26]","联机自动，步骤2，等待到达压力/位置上限"]
["M0028",null,"D0028","油缸压力反馈Mpa","FromTo","S128",null,null,null,"[27]","联机自动，步骤3，等待保压计时完成"]
["M0029",null,"D0029",null,"FromTo","S129",null,null,null,"[28]","联机自动，步骤4，等待PLC给出下降命令"]
["M0030",null,"D0030","油缸压力反馈Bar","这个用于和HMI数值比较",{"$nulls":4},"[29]","联机自动，步骤4，等待泄压计时完成"]
["M0031",null,"D0031",{"$nulls":6},"[30]","联机自动，步骤5，等待油缸到达下极限位置。"]
["M0032",null,"D0032",{"$nulls":6},"[31]","联机自动，已暂停"]
["M0033",null,"D0033",{"$nulls":6},"[32]"]
["M0034",null,"D0034","AiMpa","这两个值是浮点数",{"$nulls":4},"[33]"]
["M0035",null,"D0035",{"$nulls":6},"[34]"]
["M0036",null,"D0036","AiBar",{"$nulls":5},"[35]"]
["M0037",null,"D0037",{"$nulls":6},"[36]"]
["M0038",null,"D0038",{"$nulls":6},"[37]"]
["M0039",null,"D0039",{"$nulls":6},"[38]"]
["M0040","位移平均值采样计数>","D0040","油缸位置反馈AD","RD3A",{"$nulls":4},"[39]"]
["M0041","位移平均值采样计数=","D0041",null,"RD3A",{"$nulls":4},"[40]","请打开液压张电机"]
["M0042","位移平均值采样计数<","D0042","油缸位置反馈Float","RD3A",{"$nulls":4},"[41]","请选择合法的操作模式"]
["M0043",null,"D0043","油缸位置反馈Float","RD3A"]
["M0044",null,"D0044",null,"RD3A",{"$nulls":4},"当前操作模式：D3"]
["M0045",null,"D0045",null,"RD3A",{"$nulls":4},"[0]","无模式"]
["M0046",null,"D0046",null,"RD3A",{"$nulls":4},"[1]","调整模式"]
["M0047",null,"D0047",null,"RD3A",{"$nulls":4},"[2]","手动模式"]
["M0048",null,"D0048","油缸位置反馈mm","RD3A",{"$nulls":4},"[3]","半自动模式"]
["M0049",null,"D0049","油缸位置反馈mm","RD3A",{"$nulls":4},"[4]","联机模式"]
["M0050","位移尺的值有效","D0050","油缸位移反馈AD-FromTo","FromTo"]
["M0051",null,"D0051",null,"FromTo"]
["M0052",null,"D0052","油缸位移反馈采样计数","FromTo",{"$nulls":4},"自动步骤：D100"]
["M0053",null,"D0053","油缸位移反馈采样计数","FromTo",{"$nulls":4},"[0]","尚未进入自动流程"]
["M0054",null,"D0054","油缸位移反馈AD-SUM","FromTo",{"$nulls":4},"[1]","快顶"]
["M0055",null,"D0055","油缸位移反馈AD-SUM","FromTo",{"$nulls":4},"[2]","慢顶"]
["M0056",null,"D0056","油缸位移反馈AD-Avg","FromTo",{"$nulls":4},"[3]","保压"]
["M0057",null,"D0057","油缸位移反馈AD-Avg","FromTo",{"$nulls":4},"[4]","泄压"]
["M0058",null,"D0058",null,"FromTo",{"$nulls":4},"[5]","下降"]
["M0059",null,"D0059",null,"FromTo"]
["M0060","手动上升标志位","D0060","油缸位移反馈mm","FromTo"]
["M0061","手动下降标志位","D0061","油缸位移反馈mm","FromTo",{"$nulls":4},"当前产品型号：D1000"]
["M0062",null,"D0062","Aimm","这个值是浮点数",{"$nulls":4},"[0]","型号非法"]
["M0063",null,"D0063","Aimm",{"$nulls":5},"[1]","产品型号1"]
["M0064",null,"D0064","Ai100μm","用于和HMI值比较",{"$nulls":4},"[2]","产品型号2"]
["M0065",null,"D0065",{"$nulls":6},"[3]","产品型号3"]
["M0066",null,"D0066",{"$nulls":6},"[4]","产品型号4"]
["M0067",null,"D0067",{"$nulls":6},"[5]","产品型号5"]
["M0068",null,"D0068",{"$nulls":6},"[6]","产品型号6"]
["M0069",null,"D0069"]
["M0070","调整模式慢速顶出YV","D0070","伺服实际给定压力16Bit"]
["M0071","调整模式快速顶出YV","D0071"]
["M0072","调整模式保压YA","D0072","伺服实际给定流量16Bit"]
["M0073","调整模式慢速下降YV","D0073"]
["M0074","调整模式快速下降YV","D0074","伺服实际给定压力FloatFlag"]
["M0075","调整模式泄压YV","D0075","伺服实际给定压力FloatFlag"]
["M0076","手动模式慢速顶出YV","D0076","伺服实际给定流量FloatFlag"]
["M0077","手动模式快速顶出YV","D0077","伺服实际给定流量FloatFlag"]
["M0078","手动模式保压YA","D0078","伺服实际给定压力Float"]
["M0079","手动模式慢速下降YV","D0079","伺服实际给定压力Float"]
["M0080","手动模式快速下降YV","D0080","伺服实际给定流量Float"]
["M0081","手动模式泄压YV","D0081","伺服实际给定流量Float"]
["M0082","自动模式慢速顶出YV","D0082"]
["M0083","自动模式快速顶出YV","D0083"]
["M0084","自动模式保压YA","D0084"]
["M0085","自动模式慢速下降YV","D0085"]
["M0086","自动模式快速下降YV","D0086"]
["M0087","自动模式泄压YV","D0087"]
["M0088",null,"D0088"]
["M0089",null,"D0089"]
["M0090","自动条件满足","D0090","生产计数，产品数量"]
["M0091","本地自动启动","D0091"]
["M0092","双手OK","D0092"]
["M0093",null,"D0093"]
["M0094",null,"D0094"]
["M0095",null,"D0095"]
["M0096",null,"D0096"]
["M0097",null,"D0097"]
["M0098",null,"D0098"]
["M0099","步骤非法","D0099"]
["M0100","步骤合法","D0100","自动步骤的当前步"]
["M0101","自动步1快升","D0101"]
["M0102","自动步2慢升","D0102"]
["M0103","自动步3保压","D0103"]
["M0104","自动步4泄压","D0104"]
["M0105","自动步5下降","D0105"]
["M0106",null,"D0106"]
["M0107",null,"D0107"]
["M0108",null,"D0108"]
["M0109",null,"D0109"]
["M0110",null,"D0110"]
["M0111",null,"D0111"]
["M0112",null,"D0112"]
["M0113",null,"D0113"]
["M0114",null,"D0114"]
["M0115",null,"D0115"]
["M0116",null,"D0116"]
["M0117",null,"D0117"]
["M0118",null,"D0118"]
["M0119",null,"D0119"]
["M0120",null,"D0120"]
["M0121",null,"D0121"]
["M0122",null,"D0122"]
["M0123",null,"D0123"]
["M0124",null,"D0124"]
["M0125",null,"D0125"]
["M0126",null,"D0126"]
["M0127",null,"D0127"]
["M0128",null,"D0128"]
["M0129",null,"D0129"]
["M0130",null,"D0130"]
["M0131",null,"D0131"]
["M0132",null,"D0132"]
["M0133",null,"D0133"]
["M0134",null,"D0134"]
["M0135",null,"D0135"]
["M0136",null,"D0136"]
["M0137",null,"D0137"]
["M0138",null,"D0138"]
["M0139",null,"D0139"]
["M0140",null,"D0140"]
["M0141",null,"D0141"]
["M0142",null,"D0142"]
["M0143",null,"D0143"]
["M0144",null,"D0144"]
["M0145",null,"D0145"]
["M0146",null,"D0146"]
["M0147",null,"D0147"]
["M0148",null,"D0148"]
["M0149",null,"D0149"]
["M0150",null,"D0150"]
["M0151",null,"D0151"]
["M0152",null,"D0152"]
["M0153",null,"D0153"]
["M0154",null,"D0154"]
["M0155",null,"D0155"]
["M0156",null,"D0156"]
["M0157",null,"D0157"]
["M0158",null,"D0158"]
["M0159",null,"D0159"]
["M0160",null,"D0160"]
["M0161",null,"D0161"]
["M0162",null,"D0162"]
["M0163",null,"D0163"]
["M0164",null,"D0164"]
["M0165",null,"D0165"]
["M0166",null,"D0166"]
["M0167",null,"D0167"]
["M0168",null,"D0168"]
["M0169",null,"D0169"]
["M0170",null,"D0170","伺服当前压力设定值"]
["M0171",null,"D0171"]
["M0172",null,"D0172","伺服当前流量设定值"]
["M0173",null,"D0173"]
["M0174",null,"D0174"]
["M0175",null,"D0175"]
["M0176",null,"D0176"]
["M0177",null,"D0177"]
["M0178",null,"D0178"]
["M0179",null,"D0179"]
["M0180","油缸手动压力上极限","D0180","手动模式油缸压力设定Mpa","油缸上升时，因为产品型号原因区分自动参数和手动参数\n油缸下降时，手/自动使用相同的参数。\n\n保压和上升过程放一起\n泄压和下降过程放一起\n\n调整模式下全程慢速，没有保压、泄压过程。"]
["M0181","油缸手动保压时间到达","D0181","手动模式油缸保压时间设定s"]
["M0182","油缸自动压力上极限","D0182","自动模式油缸压力设定Mpa"]
["M0183","油缸自动保压时间到达","D0183","自动模式油缸保压时间设定s"]
["M0184","油缸手动位置上极限","D0184","手动模式油缸停止顶出位置设定mm"]
["M0185","油缸手动慢速上升位置","D0185","手动模式油缸减速顶出位置设定mm"]
["M0186","油缸自动位置上极限","D0186","自动模式油缸停止顶出位置设定mm"]
["M0187","油缸自动慢速上升位置","D0187","自动模式油缸减速顶出位置设定mm"]
["M0188","油缸快速下降位置","D0188","油缸快速下降位置设定mm","这两个值就是为了获取【油缸快速下降】这个M点位。这个M点位在油缸下降行程区间\n和【油缸慢速下降】这个M点位的逻辑条件互斥"]
["M0189","油缸减速下降位置","D0189","油缸减速下降位置设定mm"]
["M0190","油缸位置下极限","D0190","油缸停止下降位置设定mm"]
["M0191","手动模式泄压完成","D0191","手动模式泄压时间s"]
["M0192","自动模式泄压完成","D0192","自动模式泄压时间s"]
["M0193",null,"D0193"]
["M0194",null,"D0194"]
["M0195",null,"D0195"]
["M0196",null,"D0196"]
["M0197",null,"D0197"]
["M0198",null,"D0198"]
["M0199",null,"D0199"]
["M0200","手动模式油缸压力到达设定值","D0200","手动模式型号1油缸压力设定"]
["M0201","手动模式油缸保压时间到","D0201","手动模式型号1油缸保压时间设定"]
["M0202",null,"D0202","手动模式型号2油缸压力设定"]
["M0203",null,"D0203","手动模式型号2油缸保压时间设定"]
["M0204",null,"D0204","手动模式型号3油缸压力设定"]
["M0205",null,"D0205","手动模式型号3油缸保压时间设定"]
["M0206",null,"D0206","手动模式型号4油缸压力设定"]
["M0207",null,"D0207","手动模式型号4油缸保压时间设定"]
["M0208",null,"D0208","手动模式型号5油缸压力设定"]
["M0209",null,"D0209","手动模式型号5油缸保压时间设定"]
["M0210",null,"D0210","手动模式型号6油缸压力设定"]
["M0211",null,"D0211","手动模式型号6油缸保压时间设定"]
["M0212",null,"D0212"]
["M0213",null,"D0213"]
["M0214",null,"D0214"]
["M0215",null,"D0215"]
["M0216",null,"D0216"]
["M0217",null,"D0217"]
["M0218",null,"D0218"]
["M0219",null,"D0219"]
["M0220","自动模式步骤1压力值到达设定值","D0220","自动模式型号1步骤1油缸压力设定"]
["M0221","自动模式步骤1保压时间到达设定值","D0221","自动模式型号1步骤1油缸保压时间设定"]
["M0222","自动模式步骤2压力值到达设定值","D0222","自动模式型号1步骤2油缸压力设定"]
["M0223","自动模式步骤2保压时间到达设定值","D0223","自动模式型号1步骤2油缸保压时间设定"]
["M0224","自动模式步骤3压力值到达设定值","D0224","自动模式型号1步骤3油缸压力设定"]
["M0225","自动模式步骤3保压时间到达设定值","D0225","自动模式型号1步骤3油缸保压时间设定"]
["M0226",null,"D0226","自动模式型号2步骤1油缸压力设定"]
["M0227",null,"D0227","自动模式型号2步骤1油缸保压时间设定"]
["M0228",null,"D0228","自动模式型号2步骤2油缸压力设定"]
["M0229",null,"D0229","自动模式型号2步骤2油缸保压时间设定"]
["M0230",null,"D0230","自动模式型号2步骤3油缸压力设定"]
["M0231",null,"D0231","自动模式型号2步骤3油缸保压时间设定"]
["M0232",null,"D0232","自动模式型号3步骤1油缸压力设定"]
["M0233",null,"D0233","自动模式型号3步骤1油缸保压时间设定"]
["M0234",null,"D0234","自动模式型号3步骤2油缸压力设定"]
["M0235",null,"D0235","自动模式型号3步骤2油缸保压时间设定"]
["M0236",null,"D0236","自动模式型号3步骤3油缸压力设定"]
["M0237",null,"D0237","自动模式型号3步骤3油缸保压时间设定"]
["M0238",null,"D0238","自动模式型号4步骤1油缸压力设定"]
["M0239",null,"D0239","自动模式型号4步骤1油缸保压时间设定"]
["M0240",null,"D0240","自动模式型号4步骤2油缸压力设定"]
["M0241",null,"D0241","自动模式型号4步骤2油缸保压时间设定"]
["M0242",null,"D0242","自动模式型号4步骤3油缸压力设定"]
["M0243",null,"D0243","自动模式型号4步骤3油缸保压时间设定"]
["M0244",null,"D0244","自动模式型号5步骤1油缸压力设定"]
["M0245",null,"D0245","自动模式型号5步骤1油缸保压时间设定"]
["M0246",null,"D0246","自动模式型号5步骤2油缸压力设定"]
["M0247",null,"D0247","自动模式型号5步骤2油缸保压时间设定"]
["M0248",null,"D0248","自动模式型号5步骤3油缸压力设定"]
["M0249",null,"D0249","自动模式型号5步骤3油缸保压时间设定"]
["M0250",null,"D0250","自动模式型号6步骤1油缸压力设定"]
["M0251",null,"D0251","自动模式型号6步骤1油缸保压时间设定"]
["M0252",null,"D0252","自动模式型号6步骤2油缸压力设定"]
["M0253",null,"D0253","自动模式型号6步骤2油缸保压时间设定"]
["M0254",null,"D0254","自动模式型号6步骤3油缸压力设定"]
["M0255",null,"D0255","自动模式型号6步骤3油缸保压时间设定"]
["M0256",null,"D0256"]
["M0257",null,"D0257"]
["M0258",null,"D0258"]
["M0259",null,"D0259"]
["M0260","手动模式油缸位置到达顶出停止设定值","D0260","手动模式型号1油缸停止顶出位置设定"]
["M0261","手动模式油缸位置到达顶出减速设定值","D0261","手动模式型号1油缸减速顶出位置设定"]
["M0262",null,"D0262","手动模式型号2油缸停止顶出位置设定"]
["M0263",null,"D0263","手动模式型号2油缸减速顶出位置设定"]
["M0264",null,"D0264","手动模式型号3油缸停止顶出位置设定"]
["M0265",null,"D0265","手动模式型号3油缸减速顶出位置设定"]
["M0266",null,"D0266","手动模式型号4油缸停止顶出位置设定"]
["M0267",null,"D0267","手动模式型号4油缸减速顶出位置设定"]
["M0268",null,"D0268","手动模式型号5油缸停止顶出位置设定"]
["M0269",null,"D0269","手动模式型号5油缸减速顶出位置设定"]
["M0270",null,"D0270","手动模式型号6油缸停止顶出位置设定"]
["M0271",null,"D0271","手动模式型号6油缸减速顶出位置设定"]
["M0272","油缸位置到达快速下降设定值","D0272"]
["M0273","油缸位置到达减速下降设定值","D0273"]
["M0274","油缸位置到达停止下降设定值","D0274"]
["M0275",null,"D0275"]
["M0276",null,"D0276"]
["M0277",null,"D0277"]
["M0278",null,"D0278"]
["M0279",null,"D0279"]
["M0280",null,"D0280"]
["M0281",null,"D0281"]
["M0282",null,"D0282"]
["M0283",null,"D0283"]
["M0284",null,"D0284"]
["M0285",null,"D0285"]
["M0286",null,"D0286"]
["M0287",null,"D0287"]
["M0288",null,"D0288"]
["M0289",null,"D0289"]
["M0290",null,"D0290"]
["M0291",null,"D0291"]
["M0292",null,"D0292"]
["M0293",null,"D0293"]
["M0294",null,"D0294"]
["M0295",null,"D0295"]
["M0296",null,"D0296"]
["M0297",null,"D0297"]
["M0298",null,"D0298"]
["M0299",null,"D0299"]
["M0300","自动模式步骤1油缸位置到达顶出停止设定值","D0300","自动模式型号1步骤1停止顶出位置设定"]
["M0301","自动模式步骤1油缸位置到达顶出减速设定值","D0301","自动模式型号1步骤1减速顶出位置设定"]
["M0302","自动模式步骤2油缸位置到达顶出停止设定值","D0302","自动模式型号1步骤2停止顶出位置设定"]
["M0303","自动模式步骤2油缸位置到达顶出减速设定值","D0303","自动模式型号1步骤2减速顶出位置设定"]
["M0304","自动模式步骤3油缸位置到达顶出停止设定值","D0304","自动模式型号1步骤3停止顶出位置设定"]
["M0305","自动模式步骤3油缸位置到达顶出减速设定值","D0305","自动模式型号1步骤3减速顶出位置设定"]
["M0306",null,"D0306","自动模式型号2步骤1停止顶出位置设定"]
["M0307",null,"D0307","自动模式型号2步骤1减速顶出位置设定"]
["M0308",null,"D0308","自动模式型号2步骤2停止顶出位置设定"]
["M0309",null,"D0309","自动模式型号2步骤2减速顶出位置设定"]
["M0310",null,"D0310","自动模式型号2步骤3停止顶出位置设定"]
["M0311",null,"D0311","自动模式型号2步骤3减速顶出位置设定"]
["M0312",null,"D0312","自动模式型号3步骤1停止顶出位置设定"]
["M0313",null,"D0313","自动模式型号3步骤1减速顶出位置设定"]
["M0314",null,"D0314","自动模式型号3步骤2停止顶出位置设定"]
["M0315",null,"D0315","自动模式型号3步骤2减速顶出位置设定"]
["M0316",null,"D0316","自动模式型号3步骤3停止顶出位置设定"]
["M0317",null,"D0317","自动模式型号3步骤3减速顶出位置设定"]
["M0318",null,"D0318","自动模式型号4步骤1停止顶出位置设定"]
["M0319",null,"D0319","自动模式型号4步骤1减速顶出位置设定"]
["M0320",null,"D0320","自动模式型号4步骤2停止顶出位置设定"]
["M0321",null,"D0321","自动模式型号4步骤2减速顶出位置设定"]
["M0322",null,"D0322","自动模式型号4步骤3停止顶出位置设定"]
["M0323",null,"D0323","自动模式型号4步骤3减速顶出位置设定"]
["M0324",null,"D0324","自动模式型号5步骤1停止顶出位置设定"]
["M0325",null,"D0325","自动模式型号5步骤1减速顶出位置设定"]
["M0326",null,"D0326","自动模式型号5步骤2停止顶出位置设定"]
["M0327",null,"D0327","自动模式型号5步骤2减速顶出位置设定"]
["M0328",null,"D0328","自动模式型号5步骤3停止顶出位置设定"]
["M0329",null,"D0329","自动模式型号5步骤3减速顶出位置设定"]
["M0330",null,"D0330","自动模式型号6步骤1停止顶出位置设定"]
["M0331",null,"D0331","自动模式型号6步骤1减速顶出位置设定"]
["M0332",null,"D0332","自动模式型号6步骤2停止顶出位置设定"]
["M0333",null,"D0333","自动模式型号6步骤2减速顶出位置设定"]
["M0334",null,"D0334","自动模式型号6步骤3停止顶出位置设定"]
["M0335",null,"D0335","自动模式型号6步骤3减速顶出位置设定"]
["M0336",null,"D0336"]
["M0337",null,"D0337"]
["M0338",null,"D0338"]
["M0339",null,"D0339"]
["M0340",null,"D0340","伺服快顶压力设定值","液压站的额定压力25Mpa，电液伺服的额定转速1800rpm"]
["M0341",null,"D0341","伺服快顶流量设定值"]
["M0342",null,"D0342","伺服慢顶压力设定值"]
["M0343",null,"D0343","伺服慢顶流量设定值"]
["M0344",null,"D0344","伺服慢退压力设定值"]
["M0345",null,"D0345","伺服慢退流量设定值"]
["M0346",null,"D0346","伺服快退压力设定值"]
["M0347",null,"D0347","伺服快退流量设定值"]
["M0348",null,"D0348","伺服空载压力设置","伺服减退压力设定值"]
["M0349",null,"D0349","伺服空载流量设置","伺服减退流量设定值"]
["M0350",null,"D0350"]
["M0351",null,"D0351"]
["M0352",null,"D0352"]
["M0353",null,"D0353"]
["M0354",null,"D0354"]
["M0355",null,"D0355"]
["M0356",null,"D0356"]
["M0357",null,"D0357"]
["M0358",null,"D0358"]
["M0359",null,"D0359"]
["M0360",null,"D0360"]
["M0361",null,"D0361"]
["M0362",null,"D0362"]
["M0363",null,"D0363"]
["M0364",null,"D0364"]
["M0365",null,"D0365"]
["M0366",null,"D0366"]
["M0367",null,"D0367"]
["M0368",null,"D0368"]
["M0369",null,"D0369"]
["M0370",null,"D0370"]
["M0371",null,"D0371"]
["M0372",null,"D0372"]
["M0373",null,"D0373"]
["M0374",null,"D0374"]
["M0375",null,"D0375"]
["M0376",null,"D0376"]
["M0377",null,"D0377"]
["M0378",null,"D0378"]
["M0379",null,"D0379"]
["M0380",null,"D0380"]
["M0381",null,"D0381"]
["M0382",null,"D0382"]
["M0383",null,"D0383"]
["M0384",null,"D0384"]
["M0385",null,"D0385"]
["M0386",null,"D0386"]
["M0387",null,"D0387"]
["M0388",null,"D0388"]
["M0389",null,"D0389"]
["M0390",null,"D0390"]
["M0391",null,"D0391"]
["M0392",null,"D0392"]
["M0393",null,"D0393"]
["M0394",null,"D0394"]
["M0395",null,"D0395"]
["M0396",null,"D0396"]
["M0397",null,"D0397"]
["M0398",null,"D0398"]
["M0399",null,"D0399"]
["M0400","AD1CH1Bit0","D0400"]
["M0401","AD1CH1Bit1","D0401"]
["M0402","AD1CH1Bit2","D0402"]
["M0403","AD1CH1Bit3","D0403"]
["M0404","AD1CH1Bit4","D0404"]
["M0405","AD1CH1Bit5","D0405"]
["M0406","AD1CH1Bit6","D0406"]
["M0407","AD1CH1Bit7","D0407"]
["M0408","AD1CH1Bit8","D0408"]
["M0409","AD1CH1Bit9","D0409"]
["M0410","AD1CH1Bit10","D0410"]
["M0411","AD1CH1Bit11","D0411"]
["M0412","AD1CH1Bit12","D0412"]
["M0413","AD1CH1Bit13","D0413"]
["M0414","AD1CH1Bit14","D0414"]
["M0415","AD1CH1Bit15","D0415"]
["M0416",null,"D0416"]
["M0417",null,"D0417"]
["M0418",null,"D0418"]
["M0419",null,"D0419"]
["M0420","AD1CH2Bit0","D0420"]
["M0421","AD1CH2Bit1","D0421"]
["M0422","AD1CH2Bit2","D0422"]
["M0423","AD1CH2Bit3","D0423"]
["M0424","AD1CH2Bit4","D0424"]
["M0425","AD1CH2Bit5","D0425"]
["M0426","AD1CH2Bit6","D0426"]
["M0427","AD1CH2Bit7","D0427"]
["M0428","AD1CH2Bit8","D0428"]
["M0429","AD1CH2Bit9","D0429"]
["M0430","AD1CH2Bit10","D0430"]
["M0431","AD1CH2Bit11","D0431"]
["M0432","AD1CH2Bit12","D0432"]
["M0433","AD1CH2Bit13","D0433"]
["M0434","AD1CH2Bit14","D0434"]
["M0435","AD1CH2Bit15","D0435"]
["M0436",null,"D0436"]
["M0437",null,"D0437"]
["M0438",null,"D0438"]
["M0439",null,"D0439"]
["M0440",null,"D0440"]
["M0441",null,"D0441"]
["M0442",null,"D0442"]
["M0443",null,"D0443"]
["M0444",null,"D0444"]
["M0445",null,"D0445"]
["M0446",null,"D0446"]
["M0447",null,"D0447"]
["M0448",null,"D0448"]
["M0449",null,"D0449"]
["M0450",null,"D0450"]
["M0451",null,"D0451"]
["M0452",null,"D0452"]
["M0453",null,"D0453"]
["M0454",null,"D0454"]
["M0455",null,"D0455"]
["M0456",null,"D0456"]
["M0457",null,"D0457"]
["M0458",null,"D0458"]
["M0459",null,"D0459"]
["M0460",null,"D0460"]
["M0461",null,"D0461"]
["M0462",null,"D0462"]
["M0463",null,"D0463"]
["M0464",null,"D0464"]
["M0465",null,"D0465"]
["M0466",null,"D0466"]
["M0467",null,"D0467"]
["M0468",null,"D0468"]
["M0469",null,"D0469"]
["M0470",null,"D0470"]
["M0471",null,"D0471"]
["M0472",null,"D0472"]
["M0473",null,"D0473"]
["M0474",null,"D0474"]
["M0475",null,"D0475"]
["M0476",null,"D0476"]
["M0477",null,"D0477"]
["M0478",null,"D0478"]
["M0479",null,"D0479"]
["M0480",null,"D0480"]
["M0481",null,"D0481"]
["M0482",null,"D0482"]
["M0483",null,"D0483"]
["M0484",null,"D0484"]
["M0485",null,"D0485"]
["M0486",null,"D0486"]
["M0487",null,"D0487"]
["M0488",null,"D0488"]
["M0489",null,"D0489"]
["M0490","合法型号","D0490"]
["M0491","型号1已选","D0491"]
["M0492","型号2已选","D0492"]
["M0493","型号3已选","D0493"]
["M0494","型号4已选","D0494"]
["M0495","型号5已选","D0495"]
["M0496","型号6已选","D0496"]
["M0497",null,"D0497"]
["M0498",null,"D0498"]
["M0499","非法型号","D0499"]
["M0500",null,"D0500"]
["M0501",null,"D0501"]
["M0502",null,"D0502"]
["M0503",null,"D0503"]
["M0504",null,"D0504"]
["M0505",null,"D0505"]
["M0506",null,"D0506"]
["M0507",null,"D0507"]
["M0508",null,"D0508"]
["M0509",null,"D0509"]
["M0510",null,"D0510"]
["M0511",null,"D0511"]
["M0512",null,"D0512"]
["M0513",null,"D0513"]
["M0514",null,"D0514"]
["M0515",null,"D0515"]
["M0516",null,"D0516"]
["M0517",null,"D0517"]
["M0518",null,"D0518"]
["M0519",null,"D0519"]
["M0520",null,"D0520"]
["M0521",null,"D0521"]
["M0522",null,"D0522"]
["M0523",null,"D0523"]
["M0524",null,"D0524"]
["M0525",null,"D0525"]
["M0526",null,"D0526"]
["M0527",null,"D0527"]
["M0528",null,"D0528"]
["M0529",null,"D0529"]
["M0530",null,"D0530"]
["M0531",null,"D0531"]
["M0532",null,"D0532"]
["M0533",null,"D0533"]
["M0534",null,"D0534"]
["M0535",null,"D0535"]
["M0536",null,"D0536"]
["M0537",null,"D0537"]
["M0538",null,"D0538"]
["M0539",null,"D0539"]
["M0540",null,"D0540"]
["M0541",null,"D0541"]
["M0542",null,"D0542"]
["M0543",null,"D0543"]
["M0544",null,"D0544"]
["M0545",null,"D0545"]
["M0546",null,"D0546"]

{"sheet":"PLC物理地址","index":2,"n_rows":65,"n_cols":10,"rows_kept":65,"cut":false,"hidden":false,"merged":[[57,0,57,3],[60,0,60,3],[63,0,63,3]]}
["输入","触点","线圈","注释"]
["X000","*",null,"手动"]
["X001","*",null,"半自动"]
["X002","*",null,"伺服起动"]
["X003","*",null,"伺服停止",null,"常闭按钮",null,"线体急停I0.4也会触发X3","线体急停，液压站上的急停，电机停止按钮这三个条件串联接到X3"]
["X004","*",null,"慢速顶出点","慢顶","开关没接"]
["X005","*",null,"静止",null,"常闭按钮"]
["X006","*",null,"双手按钮"]
["X007","*",null,"双手按钮"]
["X010","*",null,"快退点","快退","开关没接"]
["X011","*",null,"主缸压力",null,"开关没接"]
["X012","*",null,"主缸顶出按钮"]
["X013","*",null,"主缸退回按钮"]
["X014","*",null,"液位低报警"]
["X015","*",null,"油温需冷却"]
["X016","*",null,"油温过高停机"]
["X017","*",null,"主缸顶出极限","上极限","常开触点"]
["X020","*",null,"主缸退回极限","下极限","常开触点"]
["X021"]
["X022","*",null,"减退点",null,"开关没接"]
["X023"]
["X024"]
["X025",null,null,"型号Bit0"]
["X026",null,null,"型号Bit1"]
["X027",null,null,"型号Bit2"]
["X030",null,null,"一次","来自线体","Q20.2","粉","压机1次成型","此时磨具车到位","第1次上升命令"]
["X031",null,null,"二次","来自线体","Q20.3","白","压机2次成型","此时上限位柱更换完成","第2次上升命令"]
["X032",null,null,"三次顶","来自线体","Q20.4","浅蓝","压机3次动作","此时模具车换位完成","第3次上升命令"]
["X033",null,null,"三次回","来自线体","Q20.5","灰","压机4次动作","此时压制品已经取出","退模步骤等线体夹住摸具之后再退回"]
["X034"]
["X035"]
["X036"]
["X037"]
[]
["输出","触点","线圈","注释"]
["Y000","*","*(   3 )","YA1小泵"]
["Y001",null,"*(   3 )","YA2大泵"]
["Y002","*","*(   3 )","YA3退回"]
["Y003","*","*(   2 )","YA4上行"]
["Y004","*","*(   2 )","YA5泄压"]
["Y005"]
["Y006","*","*(   1 )","电机使能"]
["Y007",null,"*(   1 )","冷却控制"]
["Y010",null,"*(   1 )","启动指示"]
["Y011"]
["Y012"]
["Y013"]
["Y014"]
["Y015",null,null,"型号Bit0"]
["Y016",null,null,"型号Bit1"]
["Y017",null,null,"型号Bit2",null,"线体点位","线色","变量说明"]
["Y020",null,"*(   1 )","一次","发给线体","I29.0","蓝","压机1次成型完成"]
["Y021",null,"*(   1 )","二次","发给线体","I29.1","红","压机2次成型完成"]
["Y022",null,"*(   1 )","三次顶","发给线体","I29.2","深蓝","退模完成，此时压机在顶出极限位置，等待夹爪夹出压制品"]
["Y023",null,"*(   1 )","三次回","发给线体","I29.3","红黑","下滑台回退完成，意思是压机在下极限位置。"]
["Y024",null,"*(   1 )","运行中","发给线体","I29.4","绿","压机运行中。"]
[]
["伺服驱动器-FX2DA"]
["流量",null,null,"PLC的AO模块发送伺服驱动器的AI"]
["压力",null,null,"PLC的AO模块发送伺服驱动器的AI"]
["油缸-FX2AD - 1"]
["压力","压力传感器"]
[]
["油缸-FX2AD - 2"]
["位移","位移传感器","行程900mm电流型","现场位移串"]